Encore™ Double 4 1/2" x 12' 1" Herringbone Dutchlap Vinyl Siding

**Specifications**

Siding Profile

Double 4-1/2" Dutchlap

Color

Herringbone

Length

12 ft. 1 in.

Thickness

0.04 inch

Material

Vinyl

Siding Surface Design

Woodgrain

Overall Width

9 inch

Overall Length

145 inch

Exposure

9 inch

Coverage Per Piece

9.06 square foot

Manufacturer Warranty

Limited Lifetime

Special Features

Class 1(A) Fire Rating

Maximum Wind Resistance

175 miles per hour

Listing Agency Standards

Class 1(A) Fire Rating